COMMENT_PUBLIC
--------------
PRIMERGY TX1320 M2 / TX1330 M2 uEFI FW changes:


uEFI FW V5.0.0.11 R1.29.0 for D3373-A1x
==============================================
Changes and problems fixed:
- Update CPU microcode to 0000F0h
- Vulnerability: Solved Intel-SA-00615. Following CVEs are addressed.
(Intel-SA-00615: CVE-2022-21123, CVE-2022-21127, CVE-2022-21125,
CVE-2022-21166)


uEFI FW V5.0.0.11 R1.28.0 for D3373-A1x
==============================================
Changes and problems fixed:
- Update CPU microcode to 0000EAh
- Update SPS FW to SPS_E3_04.01.04.306.0
- Vulnerability: Support for IPU2021.1 (Intel Platform Update).
(INTEL-SA-00463: CVE-2020-12357, CVE-2020-8670, INTEL-SA-00464:
CVE-2020-24512)
- Vulnerability: Support for Intel 2020.2 (Intel Platform Update).
(Intel-SA-00381: CVE-2020-8696, Intel-SA-00389: CVE-2020-8694, CVE-2020-8695,
Intel-SA-00391: CVE-2020-8705)
- Solved the issue that BIOS configuration backup/restore don't complete
correctly when any error happens in that processing. Added retry mechanism at
max. 3 times.
- Solved the issue that UEFI OS can boot even if all boot options are disabled.
- Improved the help message of "Active Processor Cores" shown in Help area of
BIOS setup by adding the meaning of "0".
- Changed some BIOS Setup name related to Secure Boot as below. This
modification has no effect on BIOS behavior.
Secure Boot -> Secure Boot Configuration
Secure Boot control -> Secure Boot Control
System Mode -> Platform Mode
Provision Factory Default keys -> Factory Default Key Provision
- Update LSI RAID Driver to 06010A00
- Vulnerability: Fixed CVE-2019-14575


uEFI FW V5.0.0.11 R1.27.0 for D3373-A1x
==============================================
Hint:please stop Server view agent before SLES12 SP5 ASP

Changes and problems fixed:
-BIOS settings may not be remained after replacement of system board with
old BIOS revision. Fixed to ensure restoring between old and new BIOS
revisions successfully.(SA233717720, QH200807-001)
-Solved: DIMM uncorrectable error, DIMM correctable error, and PCIe
uncorrectable error will not be logged in SEL. System might continue
to run if PCIe uncorrectable error was occurred.
*Caution:This issue is included in R1.24.0 -R1.26.0.
If you use those BIOS version, BIOS must be updated to 1.27.0 or later.
-In the case of IERR due to DIMM-UE, BIOS detects DIMM-UE during next boot
but continue to use the failed DIMM.
Solved to reset and disables failed DIMM when BIOS detects DIMM-UE during boot.
-Network Stack setting is not restored via SNTCI because this is excluded
from backup/restore. Added to backup/restore target. (SA233725375)
-NMI is not issued when memory uncorrectable error and PCI uncorrectable
error are detected.
Solved to issue NMI when memory uncorrectable error and PCI uncorrectable
error are detected, so that OS may be able to handle uncorrectable error event.


uEFI FW V5.0.0.11 R1.25.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Integration of Intel QSR 2020.1 update (CVE-2020-0594, CVE-2020-0595,
CVE-2020-0586, CVE-2020-0542, CVE-2020-0596, CVE-2020-0538, CVE-2020-0534,
CVE-2020-0533, CVE-2020-0566, CVE-2020-0532, CVE-2020-0541, CVE-2020-0597,
CVE-2020-0531, CVE-2020-0535, CVE-2020-0540, CVE-2020-0536, CVE-2020-0537,
CVE-2020-0545, CVE-2020-8674, CVE-2020-0539)

- RX25x0M1 : BIOSenters deadloop if PCI Confg Read to non-existent device.
- TX13x0M3 : The Slot number of PCIe UE SEL is incorrectly recorded when
CPU PCI bridge detects PCI UE.


uEFI FW V5.0.0.11 R1.24.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Integration of Intel QSR 2019.2 Q2 update (CVE-2019-0117, CVE-2019-0123,
CVE-2019-0124, CVE-2019-0169, CVE-2019-11132, CVE-2019-11147,
CVE-2019-11105, CVE-2019-11088, CVE-2019-11131, CVE-2019-11104,
CVE-2019-11097, CVE-2019-11103, CVE-2019-0131, CVE-2019-11090,
CVE-2019-0165,  CVE-2019-0166, CVE-2019-0168, CVE-2019-11087,
CVE-2019-11101, CVE-2019-11100,CVE-2019-11102,CVE-2019-11106,
CVE-2019-11107, CVE-2019-11109,CVE-2019-11110,CVE-2019-11086,
CVE-2019-11108, CVE-2019-0185, CVE-2019-0154)

- Resolved an issue of PCI error at POST after PCI slot status change.
- Minor bug fix


uEFI FW V5.0.0.11 R1.23.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 000000CCh
- Integration of Intel QSR 2019.1 update (CVE-2019-0086, CVE-2019-0089,
CVE-2019-0090, CVE-2019-0091, CVE-2019-0092, CVE-2019-0093, CVE-2019-0094,
CVE-2019-0096, CVE-2019-0097, CVE-2019-0098, CVE-2019-0099, CVE-2019-0153,
CVE-2019-0170, CVE-2018-12126, CVE-2018-12127, CVE-2018-12130)
- Integration of fix for Intel Transactional Synchronization Extensions (TSX)
Memory Ordering Issue
- Integration of Intel DCI Policy Update (CVE-2018-3652)
- Fixed an issue that led to random occurences of POST message
"POST - No memory installed" during system startup
- Fixed doubled boot options with RedHat 7.5 installed in UEFI mode


uEFI FW V5.0.0.11 R1.22.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 000000C6h
- Update to Intel SPS FW SPS_E3_04.01.04.54.0 (INTEL SA-00086)
- Fixed Side-Channel Analysis Method Vulnerability - (CVE-2018-3639,
CVE-2018-3640, INTEL SA-00115)
- Fixed an issue with incorrect system time change due to Daylight Saving


uEFI FW V5.0.0.11 R1.21.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 000000C2h
- Fix for side-channel analysis security flaws - known as Spectre & Meltdown
- Improved handling of SPI BIOS flash device


uEFI FW V5.0.0.11 R1.20.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 000000BAh
- Resolved an issue with Nvidia NVS315 GPU causing PCIe SERR error messages
being logged into iRMC SEL when Windows Server 2016 is installed


uEFI FW V5.0.0.11 R1.18.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 000000A6h
- Resolved an issue that led to a system hang up when the system was
idling in uEFI FW setup for more than 30 hours
- Resolved issues that a memory dump was not created when initiated by
pressing the NMI front panel button
- Removed a duplicate entry in uEFI setup in case a TPM module is
present in the system


uEFI FW V5.0.0.11 R1.14.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Resolved highly sporadic occurrence of system being powered down after
repeated logging of error message "POST - No memory installed" /
"BIOS POST Watchdog - Action: Hard Reset (Post Code: 0x55)" in iRMC SEL
after warm reboot
- Resolved issue regarding Windows Server 2016 logo compatibility


uEFI FW V5.0.0.11 R1.13.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel Skylake Microcode ID 0000008Ah
- Support for BIOS Parameter Backup without a dedicated reboot
- Added network inventory support for Intel LAN PCIe adapters (X710-DA2,
X550-T2)
- Minor bug-fixes


uEFI FW V5.0.0.11 R1.11.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Update to Intel SPS FW E3_04.00.03.95.0 (PLR2)
- Update to Intel Skylake Microcode ID 00000084h
- Update to VGA BIOS 3.8SV (supports Windows 2016)
- Update to AVAGO EFI driver v04090000 for onboard SW-RAID
- resolved behavior that user password cannot be changed without admin
password by using eLCM RestAPI
- resolved sporadic DIMM ECC error under specific UEFI FW online update
circumstances
- resolved issue that after disabling TPM support in UEFI setup, Trusted
Computing menu disappears after next reboot
- moved password prompt during POST before OPROM scan
- resolved problem that in case of disabling a single DIMM of channel by
UEFI setup next boot ends up in a hang condition


uEFI FW V5.0.0.11 R1.10.0 for D3373-A1x
==============================================

Changes and problems fixed:
- Fixed a critical TPM handling problem during OS runtime


uEFI FW V5.0.0.11 R1.9.0 for D3373-A1x
==============================================

Changes and problems fixed:
- update to Intel SPS FW E3_04.00.03.89.0 (PRL1)
- update to Intel Skylake Microcode ID 00000074h
- removed external NIC MAC addresses from system information setup page
- resolved POST screen corruption after password prompt/legacy ROM init
- resolved unexpected ACPI messages under Linux RH7/SLES12
- resolved that PXE boot from LoM port2 can?t be established via VIOM
- resolved behavior of unexpected power on if system was powered off after
WOL before OS boot finished

New features:
- support of onboard SoftwareRAID solution (enabled uEFI FW setup switch)
- support of TPM 2.0

IMPORTANT HINT:
SoftwareRAID support requires OS driver >= V17.01.2015.0716.
In case of ServerViewRAID usage a version >= V6.3.6 is mandatory.
Both packages can be found on common FJ download path.


uEFI FW V5.0.0.11 R1.7.0 for D3373-A1x
==============================================
- Initial Release

COMMENT_CRITICAL
----------------

BIOS- or firmware updates always require a closing system reboot.
 

Important notes for Windows Operating Systems
===========================================

To enable BIOS / firmware updates, the BitLocker Drive Encryption must be temporarily disabled.
After the updates have been completed,the BitLocker Drive Encryption can be re-enabled.


Important notes for Linux Operating Systems
===========================================

XEN operating systems: 
-------------------------------------------------------
Currently BIOS updates under XEN are not supported.
To update the BIOS please boot the system in non XEN mode or use offline update from Update DVD.







COMMENT_INTERNAL  
----------------  
ASP Frame Version Windows: 04.70.33
 
PrimeUpUnzip: 6.00 
DeskFlash: 06.76-0076-UEFI 
do_deskflash: 1.0.0 
