CCNP Enterprise Core ENCOR 350-401 Complete Video Course CML^2 Topology Files

Any successful deployment of a new technology includes a solid understanding of its features and concepts.

The instructors have provided sample topology files that are built upon the Cisco Modeling Labs (CML^2). CML^2 provides a scalable, extensible network design and simulation environment and can be used for a variety of test scenarios and changes prior to deployment in a production network. It includes several Cisco Network Operating System virtual machines and has the ability to integrate with third-party-vendor virtual machines.

The topology files are provided so that you can test the concepts that were explained, and most topology files replicate the environment used during the recording of these videos. The topologies re imported via the CML^2 Lab Manager using the “IMPORT” functionality.

Happy Labbing!

Brad, Brad, and Vinit